# Haven v1.6.0

Civilized Permanence micro-UI watch face for Pebble Time 2 and Pebble Round 2.

## Identity

- Product: Haven
- Version: 1.6.0
- Company: Sligh Ltd.
- Platforms: Emery and Gabbro
- UUID: `FEBD8FF2-8DBE-496E-994F-D17158212BAC`

## v1.6.0 revision

- Integrated Complications Library 1.0.0 into the existing configurable modules without changing their defaults or geometry.
- See `COMPLICATIONS_INTEGRATION.md` for the complete geometry-compatible list and validation status.

## v1.5.0 revision

- Added a dedicated circular-safe Gabbro layout.
- Preserved the established Emery v1.4.0 geometry and fixed Rows 1, 2, and 5.
- Added Clay configuration for all Row 3 and Row 4 modules.
- BAT, SUNRISE, and SUNSET positions are mutually interchangeable.
- The primary weather field can show current temperature, humidity, precipitation chance, or US AQI.
- The compact target field can use the automatic HIGH/LOW cycle, HIGH only, or LOW only.
- Repeated wide-module selections are permitted.
- Expanded Open-Meteo delivery to include precipitation probability and US AQI.
- Retained locale-derived Fahrenheit/Celsius behavior and the Arroyo Grande fallback location.
- Retained the fixed Civilized Permanence PWR/WTR/SEC simulation row.

## Fixed interface rows

- Row 1: weekday, date, menu glyph
- Row 2: main time, seconds, AM/PM when required
- Row 5: PWR, WTR, and SEC Civilized Permanence status simulation

## Configurable module families

### Wide modules

The upper-left, lower-left, and lower-right modules can independently display:

- Battery
- Sunrise
- Sunset

Defaults remain BAT, SUNRISE, SUNSET.

### Weather module

The primary weather box can display:

- Current temperature
- Humidity
- Daily maximum precipitation probability
- United States Air Quality Index

### High/Low target

The compact target box can display:

- Automatic HIGH/LOW cycle
- HIGH only
- LOW only

## Build notes

The project requires a Pebble SDK/build environment that supports Emery and Gabbro. Final PBW compilation and device validation should be performed for both targets.
